|  |
| --- |
| Photographic Records Required–T12 Plant Inspection |
| All photographs to be taken with digital camera. (4Megapixel or greater) **with date stamp function activated**. Images to be in excess of 500kb. Additional photographs may be included. Photographs may be printed (B&W acceptable) maximum of two (2) to fill an A4page and attached to Test Records. Electronic file of the photographs is to be maintained for audit purposes. Item column refers to NZTA T12:2013 |
| **Item** | **Description** | **Tick or N/A** |
| **11.3** | Photo for Certificate.  |  |
| **11.3.1** | Chassis Number: -Vin Plate or Assigned No. |  |
| **10.3***Plant and/or Trailer and/or Transporter**as appropriate to NZTA Regulations*  | NZTA Registration Label |  |
| NZTA Load Certificate |  |
| NZTA COF/WOF showing Expiry |  |
| Dangerous Goods Signs and Labels/ Facility for changing in line with product carried |  |
| Load Restraint Certification / Plate |  |
| Load securing devices comply with Transport Regulations and Truck Loading Code*(include plate as applicable)* |  |
| Vehicle complies with Vehicle Dimensions and Mass Rule |  |
| **10.2** | Product Type Loaded *(Drum or Bag labels)* |  |
| Vehicle and product storage vessels correctly signed & / or placard. |  |
| Spill Kit Type / Quantity |  |
| Emergency Procedures are appropriate to the materials being handled. |  |
| **10.1**&**11.3.2** | Pressure Relief Valves and or Burst Disks |  |
| Certification Plate on Bead Tank |  |
| Pressure Gauge Condition / Function |  |
| Operating Positions, Catwalks and Ladders*(Include handholds as appropriate)* |  |
| Machine Guarding |  |
| Fire Extinguishers with Inspection label |  |
| Gas/Diesel fired equipment is compliant with Regulations (plate) |  |
| **11.4.8** | Photograph of TMP equipment mounted on applicator and all support vehicles. i.e. Sign(s), beacons, arrow-board(s) and communication devise |  |
| **11.5***LA Type* | Apply paint and beads on left and right side of vehicle |  |
| Cleaning device on left and right side of vehicle |  |
| **11.6***LB&LC Type* | Transverse line ability |  |
| Turning Arrow ability |  |
| **12** | Test Strip, Applicator and Testing Officer*(Include entire length of strip)* |  |
| **12.4** | Sand Clean as applicable |  |
| **14.2.1** | Start & Stop of Bead Delay Test Stripe |  |
| Profile pictures of markings on Plates. *(all schedules)* |  |