|  |  |  |
| --- | --- | --- |
| **Test #:** | **Applicator:** | **Date:** |
| Company: | Operator: |
| **Test Conditions**Track Length\_\_\_\_m. Indoor / OutdoorWeather Conditions:Surface Conditions: | **8.2.1 - Test Schedules.**1. Plain flat markings
2. Audio-tactile profile markings
3. Agglomerate / Structured markings
4. Proprietary / Licensed markings. *(not covered above)*
 |
| **Marking Material.** *(Cold Applied Plastic / Thermoplastic / Other) \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_***Brand and Type: Colour: & Batch:** |
| **Time** | **Sched / Test #** | **Run #** | **Stated Speed** | **Time *(secs)*** | **Calc speed** | **Comments / Results** | **Pass / Fail** |
|  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |
| **Intermittent Line** |  | **Bead Application (1 m Kraft paper sample)** |
| **Distance (mm)** | **Spacing** | **Delay**  |  | Weight of marking without beads (gms) |  |
| 1 |  |  | Seg |  |  | Kraft Paper |  |
| 2 |  |  | Gap |  |  |  **= Material weight** |  |
| 3 |  |  | Seg |  |  | Weight of marking with beads (gms) |  |
| 4 |  |  | Gap |  |  | Kraft Paper |  |
| 5 |  |  | Seg |  |  | Minus the Material Weight |  |
| 6 |  |  | Gap |  |  | **= Material weight & beads** |  |
| 7 |  |  | Seg |  |  | **= Beads Weight** |  |
|  |  |  |  |  |  |  Size of sample (m²) |  |
|  |  |  |  |  |  |  |  |
| Straightness: | Paint to Curb: | P22 Turn Arrow: |
|  |  |  |
| *Test Prompts* |
| 12.3 | *Continuous Line Test* | *Sand cleaning / Alignment / Bead application* |  |
| 12.4 | *Intermittent Line Test* | *Bead coverage / Dimensional tolerances.*  |  |
| 12.5 | *ATP Line Test* | *Bead coverage / Dimensional tolerances* |  |