|  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| **Test #:** | | **Applicator:** | | | | | | **Date:** | | |
| Company: | | | | | Operator: | | | | | |
| **Test Conditions**  Track Length\_\_\_\_m. Indoor / Outdoor  Weather Conditions:  Surface Conditions: | | | | | **8.2.1 - Test Schedules.**   1. Plain flat markings 2. Audio-tactile profile markings 3. Agglomerate / Structured markings 4. Proprietary / Licensed markings.  *(not covered above)* | | | | | |
| **Marking Material.** *(Cold Applied Plastic / Thermoplastic / Other) \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_*  **Brand and Type: Colour: & Batch:** | | | | | | | | | | |
| **Time** | **Sched / Test #** | **Run #** | **Stated Speed** | **Time *(secs)*** | **Calc speed** | | **Comments / Results** | | | **Pass / Fail** |
|  |  |  |  |  |  | |  | | |  |
|  |  |  |  |  |  | |  | | |  |
|  |  |  |  |  |  | |  | | |  |
|  |  |  |  |  |  | |  | | |  |
|  |  |  |  |  |  | |  | | |  |
|  |  |  |  |  |  | |  | | |  |
|  |  |  |  |  |  | |  | | |  |
|  |  |  |  |  |  | |  | | |  |
|  |  |  |  |  |  | |  | | |  |
|  |  |  |  |  |  | |  | | |  |
|  |  |  |  |  |  | |  | | |  |
|  |  |  |  |  |  | |  | | |  |
|  |  |  |  |  |  | |  | | |  |
|  |  |  |  |  |  | |  | | |  |
|  |  |  |  |  |  | |  | | |  |
|  |  |  |  |  |  | |  | | |  |
|  |  |  |  |  |  | |  | | |  |
|  |  |  |  |  |  | |  | | |  |
|  |  |  |  |  |  | |  | | |  |
|  |  |  |  |  |  | |  | | |  |
|  |  |  |  |  |  | |  | | |  |
| **Intermittent Line** | | | | |  | **Bead Application (1 m Kraft paper sample)** | | | | |
| **Distance (mm)** | | **Spacing** | | **Delay** |  | Weight of marking without beads (gms) | | |  | |
| 1 |  |  | Seg |  |  | Kraft Paper | | |  | |
| 2 |  |  | Gap |  |  | **= Material weight** | | |  | |
| 3 |  |  | Seg |  |  | Weight of marking with beads (gms) | | |  | |
| 4 |  |  | Gap |  |  | Kraft Paper | | |  | |
| 5 |  |  | Seg |  |  | Minus the Material Weight | | |  | |
| 6 |  |  | Gap |  |  | **= Material weight & beads** | | |  | |
| 7 |  |  | Seg |  |  | **= Beads Weight** | | |  | |
|  |  |  |  |  |  | Size of sample (m²) | | |  | |
|  |  |  |  |  |  |  | | |  | |
| Straightness: | | | Paint to Curb: | | | | P22 Turn Arrow: | | | |
|  | | |  | | | |  | | | |
| *Test Prompts* | | | | | | | | | | |
| 12.3 | *Continuous Line Test* | | | *Sand cleaning / Alignment / Bead application* | | | | | |  |
| 12.4 | *Intermittent Line Test* | | | *Bead coverage / Dimensional tolerances.* | | | | | |  |
| 12.5 | *ATP Line Test* | | | *Bead coverage / Dimensional tolerances* | | | | | |  |